**Above the closet cabinet SPE**

The SPE type above the closet for the manifold assembly together with the equipment connector elements, i.e., atgaisotājiem, lowering valves, pumps, etc.

The cabinet is coated with enamel, standard colour RAL 9016 (balta). The back wall is 2 holes with diameter ø 6.5 mm the assembly, as well as 2 guides manifold assembly, with the help of which you can adjust the location of the collector in the closet. Each guide equipped with two M6x 18 mm bolts with nuts and washers. The lateral walls in oval technological holes 62 x 87 mm, with nosegplāksnēm laid, and through which you can connect to a collector from the side. Single height adjust with extendible legs. The front frame is adjustable, it shall be possible to adjust the depth of the building kits.

The assortment of closets and dimensions are shown in the table below:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Skapja veids** | **Gabarīti [mm]** | | | **Durvju izmēri [mm]** | |
| **platums** | **augstums** | **dziļums** | **platums** | **augstums** |
| SPE-0 | 335 | 575-675 | 111-161 | 325 | 455 |
| SPE-1 | 435 | 575-675 | 111-161 | 425 | 455 |
| SPE-2 | 565 | 575-675 | 111-161 | 555 | 455 |
| SPE-3 | 715 | 575-675 | 111-161 | 705 | 455 |
| SPE-4 | 795 | 575-675 | 111-161 | 785 | 455 |
| SPE-5 | 965 | 575-675 | 111-161 | 955 | 455 |
| SPE-6\* | 1140 | 575-675 | 111-161 | 1130 | 455 |

\* available for order

**SPE cabinets assembly**

Check the installation space required, taking into account the position of the pipeline, as well as with the height of the floor finish material (e.g., tile, laminate, etc.). The cabinet must be installed using the assistance, taking into account the thickness of insulation, and total floor height. In the closet Aircare strain up and need to be fixed to the wall through the 2 holes on the rear wall of the closet. You need to use the appropriate to strengthen the anchorages of the wall, depending on the design. If provided for in the pipeline at the collector to add through the holes in the sides of the plate, you need to remove the cover. In order to protect the built-in oven the visible part of the damage that can occur when finishing work, there is an opportunity to dismantle the front frame and the door. Collector completed attached to existing guide screws that came with the cabinet. Collector position guide is adjusted with screw.



Tehnisko aprakstu veidojis Artūrs Ārmanis

AS Akvedukts

